TRIADA
by
blackSKYwhite

Attn Technical Director, Stage Manager

Dear Sir

    Here you can find an outline of technical requirements for Triada by blackSKYwhite theatre. To provide you by exact light plan and list of equipment to be used, we hardly need the stage plan of the theatre we will perform. Would you be so kind as to send it to me by email: drda@blackskywhite.ru.
    If you have some questions as far as it is concern to content of this outline, don’t hesitate to contact to me by email or by phone: +7 916 6055794 (mob)
 
TRIADA 
Technical requirements (sketch)
 
Stage dimensions:
Min- 8*8*6m
Optimum- 12*10*8 m
Floor- black plastic
Curtains- black box on the stage according to the plan 
Props- 7 rises 2*1*0.6m (all black covered) according to the plan  and three stairs
Light Fixtures:
                      4 Moving heads wash MAC2000wash
                      4 Moving heads spot MAC500
	          9 moving heads spot MAC2000 Profile	

Lasers- Three head white laser 5-10 wt 
Two separate DMX lines for floor and ceiling
Smoke- light smoke machine 2Kwt, manipulated from light console or near light console (DMX control). Heavy (creepy) fog machine (with converter- no dry ice), 2 hazers
Sound- CD’s or MD's
Amplification and acoustic as good as possible, sound pressure about 105db
Monitors on the stage, subwoofers on the floor, front wide range loudspeakers as high as possible 
General note- we need to control sound and lighting from one place
Montage-  8 hours for montage, 4 hours of lighting rehearsal and sound check. 
                   3 hours for dismantling
                  Duration of the performance 47 min without intermission
Special effects- no open fire, no pyrotechnics, and no strobe effects